| ES |  |  | RO

Menu

| # Grease separator ## Animal fats

Separators > Grease separator
Description The purpose of the grease separator is to separate the remains of animal and vegetable fats and detergents. It is an essential product for communities such as hotels, restaurants, bars and camp sites. The Resmat grease separator units are built to standard DIN 4040 and European standard UNE-EN 1825-2, and have a grease reduction rate of up to 90%.
MATERIAL -Fibreglass-reinforced polyester. -Polypropylene manholes. CHARACTERISTICS -High chemical and mechanical resistance. -High corrosion-resistance. -High weather-resistance. MAINTENANCE -Remove the layer of hydrocarbon every 2-3 months, and the sedimented solids once a year. OPERATION -Separation of grease by flotation.
Available models
Rectangular
Vol. (L) | L (mm.) | A (mm.) | H (mm.) | Pipe (mm.)
300 | 1.100 | 800 | 500 | 110
500 | 1.300 | 900 | 600 | 110
1.100 | 1.600 | 1.200 | 750 | 110
Cylindrical
Vol. (L) | Ø (mm.) | L (mm.) | H (mm.) | Pipe (mm.)
1.100 | 1.100 | 1.300 | 1.200 | 110
1.500 | 1.100 | 1.600 | 1.200 | 110
2.300 | 1.100 | 2.150 | 1.200 | 160
3.000 | 1.740 | - | alt 1.500 | 200
4.000 | 1.500 | 2.750 | 1.650 | 200
6.000 | 1.725 | 3.000 | 1.850 | 200
8.000 | 2.000 | 2.960 | 2.100 | 200
10.000 | 2.000 | 3.600 | 2.100 | 200
12.000 | 2.500 | 2.950 | 2.600 | 200
15.000 | 2.500 | 3.560 | 2.600 | 200
Consult us for other volumes
Operating Details The water enters the unit and first the heavier solids are decanted to settle at the bottom of the tank. At the same time, the animal fats and detergents are separated through the difference in their specific weights, which makes the detergents and fat rise to the top of the tank. The water outlet pipe is located half-way up the separator, to prevent the heavy solids (at the bottom) and the grease and detergents (at the top) from being washed through. It is very important that only grey water is piped into the grease separator
| Legal Disclaimer | Web design by Net Engineer |