| ES |  |  | RO

Menu

| # Sand separator ## Sand traps

Separators > Sand separator
Description The Resmat sand separator or sand trap is built to European standards UNE-EN 858-1 and UNE-EN 858-2 .
MATERIAL -Fibreglass-reinforced polyester. -Polypropylene manholes. CHARACTERISTICS -High chemical and mechanical resistance. -High corrosion-resistance. -High weather-resistance. MAINTENANCE -Remove the accumulated sludge every 6 months. OPERATION -Separation of sand by decanting.
Available models
Cylindrical
Vol. (m3/d) | Ø (mm.) | L (mm.) | H (mm.)
1.100 | 1.100 | 1.300 | 1.200
1.500 | 1.100 | 1.600 | 1.200
2.300 | 1.100 | 2.150 | 1.200
3.000 | 1.740 | 1.500 | 1.800
4.000 | 1.500 | 2.750 | 1.650
6.000 | 1.725 | 3.000 | 1.850
8.000 | 2.000 | 2.960 | 2.100
10.000 | 2.000 | 3.600 | 2.100
12.000 | 2.500 | 2.950 | 2.600
15.000 | 3.500 | 3.560 | 2.600
18.000 | 2.500 | 4.170 | 2.600
20.000 | 2.500 | 4.580 | 2.600
Consult us for other volumes
Operating Details The sand separator is an essential element in car washes and any application where sand is washed in that has to be separated from the water. In car washes, the unit should be installed ahead of the hydrocarbon separator. The sand is held in the bottom of the tank, while the water is taken out through the top.
| Legal Disclaimer | Web design by Net Engineer |