| ES |  |  | RO

Menu

| # Module for early ## weaning of piglets

Livestock > Module for early weaning of piglets
The module is designed for early weaning of piglets from 6 to 20 or 22 Kg. It is designed to house the animals from 20 to 60 days, keeping the piglets safe from infection and contagion.
Features and advantages *No site license needed. *Weaning sheds can be turned into farrowing sheds, with weaning moved outdoors using the modules. *Early weaning between 20 and 60 days. *Outdoor installation. *Supports temperatures from -16ºC to 35ºC. *Savings in costly shed construction. *Fast washing with water or steam lance. *Prevention of infections and contagion. *Reduced investment costs. *Shorter pay-back time. *Transformation: 1.2 kg of feed = 1 kg of meat. *Each module can house up to 540 piglets a year. *Each module incorporates an extractor, heating, digital temperature control unit and ventilation, hopper and basing troughs. *On demand, the module can be supplied with inner and outer division, ideal for adapting it to any need.
Building an installation *Installation of the module with a 3% gradient towards the pit. *Pit covered so as not to increase purines. *PVC plastic slats. *Open-fence installation with closed ends, 2 m high. *Easy water and electricity installation.
Characteristics of the materials used *8 mm polyurethane. OM-42. *Synthetic material. *Tungsten powder. *Resistant to changes in weather. *Stainless steel bolts. *Adjustable heating. *Consumption 120W/220V. *60W extractor. Approved by the EC STANDARDS UNE_EN 60335-1 and UNE 20-458-88 PART 2-90
Average weaning results
Phase | Week | Days | Weight | CR | ADG
WEANING | 3 | 21 | 6 | - | -
3 | 23 | 6,5 | - | -
3 | 25 | 7,5 | - | -
3 | 30 | 8,5 | - | -
PRE-INITIAL | 5 | 35 | 10 | 1,16 | 320
6 | 42 | 12 | 1,20 | 330
INITIAL | 7 | 49 | 14,5 | 1,25 | 340
8 | 56 | 17,5 | 1,35 | 360
9 | 63 | 21 | 1,40 | 400
10 | 70 | 25 | 1,45 | 430
Accessories: Temperature regulation unit IPC-55 Extractor Basin drinking troughs
| Legal Disclaimer | Web design by Net Engineer |