| ES |  |  | RO

Menu

| # Drinking water tanks

Water > Drinking water tanks
## Drinking water tanks
MATERIAL -Fibreglass-reinforced polyester. -Polypropylene manholes. | CHARACTERISTICS -High chemical and mechanical resistance. -High corrosion-resistance. -High weather-resistance.
Available models
Rectangular, overground
Vol. (L) | L (mm.) | A (mm.) | H (mm.)
100 | 640 | 530 | 500
200 | 950 | 650 | 500
300 | 1.100 | 800 | 500
500 | 1.300 | 900 | 600
1.000 | 1.600 | 1.200 | 750
Consult us for other volumes
Cylindrical, overground
Vol. (L) | L (mm.) | A (mm.) | H (mm.)
100 | 640 | 530 | 500
200 | 950 | 650 | 500
300 | 1.100 | 800 | 500
500 | 1.300 | 900 | 600
1.000 | 1.600 | 1.200 | 750
Consult us for other volumes
Cylindrical, underground
Vol. (L) | Ø (mm.) | H (mm.)
200 | 600 | 1.150
300 | 740 | 1.150
500 | 940 | 1.150
1.000 | 1.120 | 1.650
2.000 | 1.490 | 1.650
3.000 | 1.740 | 1.750
Consult us for other volumes
Rectangular, underground
Vol. (L) | L (mm.) | A (mm.) | H (mm.)
100 | 640 | 530 | 500
200 | 950 | 650 | 500
300 | 1.100 | 800 | 500
500 | 1.300 | 900 | 600
1.000 | 1.600 | 1.200 | 750
Consult us for other volumes
| Legal Disclaimer | Web design by Net Engineer |