| ES |  |  | RO

Menu

| # Rain water collection tanks

Water > Rain water collection tanks
## Rain water collection tanks These tanks are designed to collect rain water. To install the tanks, you will need to channel the pipes from roofs and terraces towards the tank. There is a filter to prevent particles of over 0.55 mm getting in. This prevents leaves, sand, bird droppings, etc. from getting into the tank. If particles of this type did get into a tank with still water, it would lead to problems with odours and decomposition of the organic matter.
MATERIAL -Fibreglass-reinforced polyester. -Polypropylene manholes. | CHARACTERISTICS -High chemical and mechanical resistance. -High corrosion-resistance. -High weather-resistance.
## Garden rainwater collection tanks Rainwater collection tank, with garden type filter, with filter capacity of up to 0.55 mm. The particles retained are held in a stainless steel basket, which can easily be removed for cleaning.
Use
- Catchment area of 150-200 m2. - Catchment surface with no nearby trees. - No connection to the sewage mains.
Available models
Vol. (L) | Ø (mm.) | L (mm.) | Pipe (mm.) | Filter (model)
2.000 | 1.100 | 2.150 | 110 | Garden Filter
3.000 | 1.725 | 1.500 Alt. | 110 | Garden Filter
3.500 | 1.100 | 3.700 | 110 | Garden Filter
4.000 | 1.500 | 2.750 | 110 | Garden Filter
5.000 | 1.625 | 2.500 | 110 | Garden Filter
6.000 | 1.725 | 3.000 | 110 | Garden Filter
8.000 | 1.600 | 4.269 | 110 | Garden Filter
8.000 | 2.000 | 2.960 | 110 | Garden Filter
10.000 | 2.000 | 3.500 | 110 | Garden Filter
12.000 | 2.000 | 4.143 | 110 | Garden Filter
15.000 | 2.000 | 5.400 | 110 | Garden Filter
15.000 | 2.500 | 3.570 | 110 | Garden Filter
18.000 | 2.500 | 4.200 | 110 | Garden Filter
20.000 | 2.500 | 4.580 | 110 | Garden Filter
25.000 | 2.500 | 5.600 | 110 | Garden Filter
30.000 | 2.500 | 6.620 | 110 | Garden Filter
35.000 | 2.500 | 7.700 | 110 | Garden Filter
40.000 | 2.500 | 8.700 | 110 | Garden Filter
45.000 | 2.500 | 9.700 | 110 | Garden Filter
50.000 | 2.500 | 10.700 | 110 | Garden Filter
The tanks can be supplied with 2 different kits: Kit 1 2-3 manholes 1 PVC 110 inlet 1 PVC 110 overflow spout 1 outlet for suction pump, 2" Kit 2 Accessories kit 1 FCI filter incorporated in the tank Anti-turbulence inlet
## FCI rainwater collection tanks Rainwater collection tank, with FCI type filter, with filter capacity of up to 0.55 mm. Any leaves and particles trapped are discharged directly into the sewage mains. Use
- Catchment area of 150-200 m2. - Catchment surface where there are nearby trees. - Connection to the sewage mains. |
Available models
Vol. (L) | Ø (mm.) | L (mm.) | Pipe (mm.) | Filter (model)
2.000 | 1.100 | 2.150 | 110 | Int. Fci
3.000 | 1.725 | 1.500 Alt. | 110 | Int. Fci
3.500 | 1.100 | 3.700 | 110 | Int. Fci
4.000 | 1.500 | 2.750 | 110 | Int. Fci
5.000 | 1.625 | 2.500 | 110 | Int. Fci
6.000 | 1.725 | 3.000 | 110 | Int. Fci
8.000 | 1.600 | 4.269 | 110 | Int. Fci
8.000 | 2.000 | 2.960 | 110 | Int. Fci
10.000 | 2.000 | 3.500 | 110 | Int. Fci
12.000 | 2.000 | 4.143 | 110 | Int. Fci
15.000 | 2.000 | 5.400 | 110 | Int. Fci
15.000 | 2.500 | 3.570 | 110 | Int. Fci
18.000 | 2.500 | 4.200 | 110 | Int. Fci
20.000 | 2.500 | 4.580 | 110 | Int. Fci
25.000 | 2.500 | 5.600 | 110 | Int. Fci
30.000 | 2.500 | 6.620 | 110 | Int. Fci
35.000 | 2.500 | 7.700 | 110 | Int. Fci
40.000 | 2.500 | 8.700 | 110 | Int. Fci
45.000 | 2.500 | 9.700 | 110 | Int. Fci
50.000 | 2.500 | 10.700 | 110 | Int. Fci
The tanks can be supplied with 2 different kits: Kit 1 2-3 manholes 1 PVC 110 inlet 1 PVC 110 overflow spout 1 outlet for suction pump, 2" Kit 2 Accessories kit 1 FCI filter incorporated in the tank Anti-turbulence inlet
## HOF rainwater collection tanks
Available models
Vol. (L) | Ø (mm.) | L (mm.) | Pipe (mm.) | Filter (model)
2.000 | 1.100 | 2.150 | 110 | Ext. FGC
3.000 | 1.725 | 1.500 Alt. | 110 | Ext. FGC
3.500 | 1.100 | 3.700 | 110 | Ext. FGC
4.000 | 1.500 | 2.750 | 110 | Ext. FGC
5.000 | 1.625 | 2.500 | 110 | Ext. FGC
6.000 | 1.725 | 3.000 | 110 | Ext. FGC
8.000 | 1.600 | 4.269 | 110 | Ext. FGC
8.000 | 2.000 | 2.960 | 110 | Ext. FGC
10.000 | 2.000 | 3.500 | 110 | Ext. FGC
12.000 | 2.000 | 4.143 | 110 | Ext. FGC
15.000 | 2.000 | 5.400 | 110 | Ext. FGC
15.000 | 2.500 | 3.570 | 110 | Ext. FGC
18.000 | 2.500 | 4.200 | 110 | Ext. FGC
20.000 | 2.500 | 4.580 | 110 | Ext. FGC
25.000 | 2.500 | 5.600 | 110 | Ext. FGC
30.000 | 2.500 | 6.620 | 110 | Ext. FGC
35.000 | 2.500 | 7.700 | 110 | Ext. FGC
40.000 | 2.500 | 8.700 | 110 | Ext. FGC
45.000 | 2.500 | 9.700 | 110 | Ext. FGC
50.000 | 2.500 | 10.700 | 110 | Ext. FGC
The tanks can be supplied with 2 different kits: Kit 1 2-3 manholes 1 PVC 110 inlet 1 PVC 110 overflow spout 1 outlet for suction pump, 2" Kit 2 Accessories kit 1 FCI filter incorporated in the tank Anti-turbulence inlet
Functions included in all models Manhole: For access to and maintenance on the various tank components. Anti-turbulence inlet: The water inlet is through the bottom of the tank, preventing turbulence in the water and sedimented solids. The construction type also facilitates oxidation in the tank, thus preventing unpleasant odours. Overflow spout: Overflow spout incorporated, for removing excess water. It is designed to remove the surface sheet of water from the tank, thus helping to remove any suspended pollen that might have got in. It also stops rodents from getting in and the siphon-shape stops unpleasant odours from getting back.
Accessories: Floating suction device Large capacity filter Backwashing kit for FCI filter Ballcock + electric valve Pumps
| Legal Disclaimer | Web design by Net Engineer |