| ES |  |  | RO

Menu

| # Screen

Pre-treatment > Screen
The purpose of the screen is to retain the large bodies carried along with the waste water, which can hinder operation of the treatment equipment. The system consists of a GRP (fibreglass-reinforced polyester) tank with a protrusion screen with 25x25 mm opening for retaining the foreign bodies.
MATERIAL -Fibreglass-reinforced polyester. -Polypropylene manholes. CHARACTERISTICS -High chemical and mechanical resistance. -High corrosion-resistance. -High weather-resistance. MAINTENANCE -Remove the retained solids regularly. OPERATION -Separation of bulky bodies from waste water.
Available models
Rectangulares
Vol. (L) | L (mm.) | W (mm.) | H (mm.)
300 | 1.100 | 800 | 500
500 | 1.300 | 900 | 600
1.000 | 1.600 | 1.200 | 750
Consult us for other volumes
Operating Details Depending on the water flow to be treated we also have AUTOMATIC CIRCULAR SCREENS and SPIRAL SCREENS.
| Legal Disclaimer | Web design by Net Engineer |