| ES |  |  | RO

Menu

| # Drinking water vats

Water > Drinking water vats
## Drinking water vats
MATERIAL -Fibreglass-reinforced polyester. -Polypropylene manholes. | CHARACTERISTICS -High chemical and mechanical resistance. -High corrosion-resistance. -High weather-resistance.
All cisterns include: -1 Manhole. -2 water inlet and outlet nozzles. -1 Vent. Any type of optional accessory can be added to the vats to order
Available models
Overground Horizontal
Vol. (L) | Ø (mm.) | L (mm.)
2.000 | 1.100 | 2.150
4.000 | 1.500 | 2.750
5.000 | 1.625 | 2.500
6.000 | 1.725 | 3.000
Consult us for other volumes
Underground Horizontal
Vol. (L) | Ø (mm.) | L (mm.)
2.000 | 1.100 | 2.150
4.000 | 1.500 | 2.750
5.000 | 1.625 | 2.500
6.000 | 1.725 | 3.000
Consult us for other volumes
Overground Vertical
Vol. (L) | Ø (mm.) | H (mm.)
4.000 | 1.500 | 2.750
5.000 | 1.625 | 2.500
6.000 | 1.725 | 3.000
Consult us for other volumes
Underground Vertical
Vol. (L) | Ø (mm.) | H (mm.)
4.000 | 1.500 | 2.750
5.000 | 1.625 | 2.500
6.000 | 1.725 | 3.000
Consult us for other volumes
| Legal Disclaimer | Web design by Net Engineer |