| ES |  |  | RO

Menu

| # Hydrocarbon separator ## Coalescent with blinding

Separators > Hydrocarbon separator
Description The hydrocarbon separator is necessary in all types of vehicles and machinery workshops, garages, service stations, car washes, scrap yards, etc. The purpose of the separator is to separate up the remains of mineral grease, oils, fuels, etc. Resmat hydrocarbon separator units are built to standard DIN 1999 and European standard UNE-EN 858-1 and UNE-EN 858-2, and have a reduction rate of up to 90 %. Maximum discharged 5 mg/L.
MATERIAL -Fibreglass-reinforced polyester. -Polypropylene manholes. CHARACTERISTICS -High chemical and mechanical resistance. -High corrosion-resistance. -High weather-resistance. MAINTENANCE -Remove the layer of hydrocarbon every 2-3 months, and the sedimented solids once a year. OPERATION -Preliminary settling of solids. -Coalescence, binding of microparticles to larger drops. -Rapid flotation of the drops formed. -Blinding to prevent the hydrocarbons flowing out.
Available models
Rectangular
Vol. (L) | Flow (L/s) | L (mm.) | A (mm.) | H (mm.) | Pipe (mm.)
500 | 1,5 | 1.300 | 900 | 600 | 110
1.000 | 3 | 1.600 | 1.200 | 750 | 110
Cylindrical
Vol. (L) | Flow (L/s) | Ø (mm.) | L (mm.) | Pipe (mm.)
1.000 | 3 | 1.100 | 1.300 | 110
1.500 | 4,5 | 1.100 | 1.600 | 110
2.000 | 6 | 1.100 | 2.150 | 110
3.000 | 10 | 1.720 | alt. 1.500mm | 160
4.000 | 12 | 1.500 | 2.750 | 200
6.000 | 20 | 1.725 | 3.000 | 200
Consult us for other volumes
Operating Details The process begins with the decanting of the heavy materials, normally sand. As a result of the difference in specific weights between the water and the hydrocarbons, they move to the bottom and top of the tank respectively. The water is collected from the bottom of the tank and piped to the next chamber by means of coalescence, where the small drops of hydrocarbon, not separated in the first chamber due to their small volume, bind together to form larger drops. The last process involves the blinding buoy, whose purpose is to prevent the hydrocarbons getting out and to block the outlet if the maximum retention capacity is exceeded. In carwashes or in situations where discharges of hydrocarbons are accompanied by a large quantity of sand, it is essential to install a sand separator for the separator to work properly.
| Legal Disclaimer | Web design by Net Engineer |