| ES |  |  | RO

Menu

| # Pump shafts

|  | Catálogo |

Water > Pump shafts
## Pump shafts The pump shafts are used for water pumps that are below the drain level and cannot be gravity-drained. There are various models available depending on the specific needs.
Raised manholes Clean water pump shafts 1 pump 2 alternating pumps Foul water pump shafts 1 pump 2 alternating pumps Pump shafts with no accessories
## Raised manholes Raised manholes are normally used to drain the water from single-dwelling home treatment plants, i.e. a very simple pumping system consisting of an underground tank of the required capacity, incorporating a pump with an automatic level switch.
Standard models
Vol. (L) | Ø Pipe (mm.) | Ø (mm.) | Height (mm.) | Ø Manhole (mm.) | Ref.
300 | 110 | 740 | 1.000 | 454 | AE-300-110
300 | 125 | 740 | 1.000 | 454 | AE-300-125
500 | 125 | 940 | 1.000 | 454 | AE-500-125
500 | 160 | 940 | 1.000 | 454 | AE-500-160
500 | 200 | 940 | 1.000 | 454 | AE-500-200
1.000 | 200 | 1.120 | 1.400 | 454 | AE-1000-200
1.000 | 250 | 1.120 | 1.400 | 454 | AE-1000-250
Consult us for other volumes and measurements. Alternative diameters of pipes, pump models, etc. are available.
Characteristics of the pump in the raised manholes
Ref. | Pow. | Tens. | µF | discharge Ø | Pas. of solids
V600 | 0,8 KW | 230v | 10 | 1 ¼" | 24mm
l/min | 10 | 25 | 50 | 75 | 100 | 125 | 150 | 190 | 240
m3/h | 0,6 | 1,5 | 3 | 4,5 | 6 | 7,8 | 9 | 11,4 | 14,4
m.c.a. | 7,7 | 7,5 | 7 | 6,3 | 5,6 | 5 | 4,3 | 3 | 1
Check the pump's operating curve against the working point required in your application. The pumps can be changed as required.
## Clean water pump shafts These units are use to pump clean water; we have 2 models, with 1 or 2 pumps.
Clean water pump shaft 1 pump Characteristics: High-strength GRP tank. Inlet and outlet pipes in PVC 110,125,160,200, etc. Ventilation pipes. 1 unit. Clean water pump. 1 PVC check valve of same diameter as the pump boost diameter. 1 magnetic rod level sensor with 2 contacts. Pump start/stop circuit board with acoustic/light alarm signalling. Stainless steel chain for lowering the pump into the tank. Flexible pipes for putting the pumps in place without needing to enter the tank. Manhole Ø 620 mm.
Clean water pump shaft 2 pumps Characteristics: High-strength GRP tank. Inlet and outlet pipes in PVC 110,125,160,200, etc. Ventilation pipes. 2 unit. Clean water pump. 2 PVC check valves of same diameter as the pump boost diameter. 1 magnetic rod level sensor with 4 contacts. Stainless steel chains for lowering pumps into tank. Flexible pipes for putting the pumps in place without needing to enter the tank. Manhole Ø620mm. Circuit board for controlling pumps, suitable for 4 levels. In the first two levels each of the pumps is started/stopped alternately, i.e. each time a pump is started up it will be different to the one activated the previous time. At the third level, the 2 pumps are started at the same time and if the water reaches Level 4, an acoustic/light alarm is activated.
Characteristics of clean water pumps
Model | Pow. | Volt. | µF | Discharge Ø | Pas. of solids
D100 | 0,7KW | 230V | 12 | 1 ¼" | 7mm
V1250 | 1,1KW | 230V | 16 | 1 ¼" | 8mm
Pump model D100
l/min | 25 | 50 | 100 | 150 | 200 | 250 | 300
m3/h | 1,5 | 3 | 6 | 9 | 12 | 15 | 18
m.c.a. | 9,2 | 9,1 | 8,7 | 7,8 | 6 | 4 | 1,8
Pump model V1250
l/min | 25 | 50 | 100 | 125 | 150 | 175 | 225 | 275
m3/h | 1,5 | 3 | 6 | 7,5 | 9 | 10,5 | 13,5 | 16,5
m.c.a. | 13,2 | 12,8 | 11,8 | 11,2 | 10,4 | 9,4 | 6,5 | 2,5
Check the pump's operating curve against the working point required in your application. The pumps can be changed as required.
Standard clean water models
Vol. (L.) | Ø (mm.) | Height (mm.) | Ø Pipes (mm.) | Mod. D100 - 1 pump | Mod. D100 - 2 pumps | Mod. V1250 - 1 pump | Mod. V1250 - 2 pumps
500 | 940 | 1.050 | 125 | PBL-500-D100 | - | PBL-500-V1250 | -
1.000 | 1.120 | 1.450 | 125 | PBL-1000-D100 | PBL2-1000-D100 | PBL-1000-V1250 | PBL2-1000-V1250
2.000 | 1.490 | 1.500 | 125 | PBL-2000-D100 | PBL2-2000-D100 | PBL-2000-V1250 | PBL2-2000-V1250
3.000 | 1.725 | 1.600 | 125 | PBL-3000-D100 | PBL2-3000-D100 | PBL-3000-V1250 | PBL2-3000-V1250
Consult us for other volumes and measurements. Alternative diameters of pipes, pump models, etc. are available.
Clean water sensors IMN TB PVC Magnetic level switch Connexion to process: PVC connection (1"1/4, 1"1/2) Electrical connection: Junction box NO contact: 120W/VA - 3A / 250VACDC NO/NC contact: 60W/VA - 1A / 230VACDC Pipe: PVC Ø 16 mm Float: PP Ø 38 x 61 mm Density: 0.65 g/cm3 Temperature: -10..+60ºC Pressure: 3 kg/cm2 Protection: IP67
## Foul water pump shafts These units are used to pump waste water, sewage, grey water and water that contains solids. There are 2 models, with 1 or 2 pumps.
Foul water pump shaft 1 pump Characteristics: High-strength GRP tank Inlet and outlet pipes in PVC 110, 125, 160, 200, etc. Ventilation pipes. 1 unit. Sewage pump. 1 PVC check valve of same diameter as the pump boost diameter. 1 magnetic rod level sensor with 2 contacts. Pump start/stop circuit board with acoustic/light alarm signalling. Stainless steel chain for lowering the pump into the tank. Flexible pipes for putting the pumps in place without needing to enter the tank. Manhole Ø 620 mm.
Foul water pump shaft 2 pumps Characteristics: High-strength GRP tank. Inlet and outlet pipes in PVC 110, 125, 160, 200, etc. Ventilation pipes. 2 unit. Sewage pump. 2 PVC check valves of same diameter as the pump boost diameter. 1 magnetic rod level sensor with 4 contacts. Stainless steel chains for lowering pumps into tank. Flexible pipes for putting the pumps in place without needing to enter the tank. Manhole Ø 620mm. Circuit board for controlling pumps, suitable for 4 levels. In the first two levels each of the pumps is started/stopped alternately, i.e. each time a pump is started up it will be different to the one activated the previous time. At the third level, the 2 pumps are started at the same time and if the water reaches Level 4, an acoustic/light alarm is activated.
Characteristics of foul water pumps
Model pump | Power | Volt. | µF | Discharge Ø | Pas. of solids
DX100 | 0,75KW | 230V | 12 | 1 ¼" | 32mm
DX200 | 1,1KW | 230V | 16 | 2" | 45mm
DX202 | 1,6KW | 230V | 16 | 2" | 45mm
Pump model DX100
l/min | 25 | 50 | 100 | 150 | 200 | 250
m3/h | 1,5 | 3 | 6 | 9 | 12 | 15
m.c.a. | 7 | 6,7 | 5,9 | 5 | 3,5 | 1,8
Pump model DX200
l/min | 50 | 100 | 250 | 300 | 400
m3/h | 3 | 6 | 15 | 18 | 24
m.c.a. | 10,8 | 9,8 | 6 | 4,6 | 2
Pump model DX202
l/min | 50 | 100 | 250 | 300 | 400 | 450 | 500
m3/h | 3 | 6 | 15 | 18 | 24 | 27 | 30
m.c.a. | 14,5 | 13,3 | 9,7 | 8,2 | 5,3 | 4 | 2,5
Check the pump's operating curve against the working point required in your application. The pumps can be changed as required.
Standard foul water models
Vol. (L.) | Ø (mm.) | Height (mm.) | Ø Pipes (mm.) | Mod. DX100 - 1 pump | Mod. DX100 - 2 pumps | Mod. DX200 - 1 pump | Mod. DX200 - 2 pumps
500 | 940 | 1.050 | 125 | PBS-500-DX100 | - | PBS-500-DX200 | -
1.000 | 1.120 | 1.450 | 125 | PBS-1000-DX100 | PBS2-1000-DX100 | PBS-1000-DX200 | PBS2-1000- DX200
2.000 | 1.490 | 1.500 | 125 | PBS-2000-DX100 | PBS2-2000-DX100 | PBS-2000-DX200 | PBS2-2000-DX200
3.000 | 1.725 | 1.600 | 125 | PBS-3000-DX100 | PBS2-3000-DX100 | PBS-3000-DX200 | PBS2-3000-DX200
Vol. (L.) | Ø (mm.) | Height (mm.) | Ø Pipes (mm.) | Mod. DX202 - 1 pump | Mod. DX202 - 2 pumps
500 | 940 | 1.050 | 125 | PBS-500-DX202 | -
1.000 | 1.120 | 1.450 | 125 | PBS-1000-DX202 | PBS2-1000-DX202
2.000 | 1.490 | 1.500 | 125 | PBS-2000-DX202 | PBS2-2000-DX202
3.000 | 1.725 | 1.600 | 125 | PBS-3000-DX202 | PBS2-3000-DX202
Consult us for other volumes and measurements. Alternative diameters of pipes, pump models, etc. are available.
Foul water sensors IMN TB PVC/INOX Magnetic level switch Connection to process: PVC connection (1"1/4, 1"1/2) Electrical connection: Junction box NO contact: 120W/VA - 3A / 250VACDC NO/NC contact: 60W/VA - 1A / 230VACDC Pipe: INOX AISI316 Ø 16 mm Float: INOX AISI316 Ø 90 mm Density: 0.70 g/cm3 Ambient temperature: -40..+125ºC Pressure: 3 kg/cm2 Protection: IP67
| Legal Disclaimer | Web design by Net Engineer |