| ES |  |  | RO

Menu

| # Grey water

Treatment > Grey water
Description This unit was designed to meet a need to re-use water. Water from showers is treated and can be reused for toilet cisterns or irrigation. We have 2 models, one for reusing water for toilet cisterns and the other for irrigation. Each of the models is available in underground and overground versions.
ADVANTAGES - Great savings in consumption of drinking water. - The model for re-use for toilet cisterns, has been developed with a new water capture system; this allows us to reduce tank volumes for locations in basements, machine rooms, car parks, etc. - The units are delivered with all the accessories required for operation (except the boost pump). - They include a compartment for storing the treated water, ready to be connected to a pump to distribute the clean water. - Low electricity consumption.
MAINTENANCE - Check the filters regularly. - Clean out excess sludge once a year. - Change the UV lamp once a year. - Check chlorine level.
INSTALLATION - In order to install this treatment system, the water lines through which the re-used water is piped must be separate. The pipes containing the water must be marked "NOT DRINKING WATER".
Model for toilet re-use
Popul. | Tank Vol. (litres) | Pipe mm. | Diam. mm. | Len. mm.
50 | 2.000 | 90 | 1.100 | 2.150
85 | 3.500 | 90 | 1.100 | 3.700
100 | 4.000 | 90 | 1.500 | 2.750
125 | 5.000 | 90 | 1.625 | 2.500
150 | 6.000 | 110 | 1.725 | 3.000
Consult us for other volumes
Model for irrigation re-use
Popul. | Irrig. flow (l/day.) | Tank vol. (litres.) | Pipes (mm.) | Diam. (mm.) | Len. (mm.)
15 | 900 | 2.000 | 90 | 1.100 | 2.150
25 | 1.600 | 3.500 | 90 | 1.100 | 3.700
30 | 1.900 | 4.000 | 90 | 1.500 | 2.750
40 | 2.400 | 5.000 | 90 | 1.625 | 2.500
45 | 2.800 | 6.000 | 110 | 1.725 | 3.000
65 | 3.900 | 8.000 | 110 | 2.000 | 2.960
80 | 4.800 | 10.000 | 110 | 2.000 | 3.600
100 | 6.000 | 12.000 | 110 | 2.500 | 3.000
125 | 7.500 | 15.000 | 110 | 2.500 | 3.600
150 | 9.000 | 18.000 | 110 | 2.500 | 4.200
Contact us
| Legal Disclaimer | Web design by Net Engineer |